| # Print Cross-dock Order Priorities (whinh6421m000) Use this session to print cross-dock order priority definitions. Related topics Cross-dock order priority Priority Definition A one or two-digit numeric value. Default value 1 (highest priority) Note This field is only available if you started this session from the Cross-dock Order Priorities (whinh6121m000) session. Priority Definition A one or two-digit numeric value. Default value 99 (lowest priority) Note This field is only available if you started this session from the Cross-dock Order Priorities (whinh6121m000) session. Print Priority Details If this check box is selected, LN prints all priorities that are contained in the selected cross-dock order priority definitions. Note This field is only available if you started this session from the Cross-dock Order Priority Definitions (whinh6120m000) session. |