| # Line Segment - Stations (tiasl1550m000) Use this session to display or modify the line stations of an assembly line segment and their relationship to each other. You can display the current effective stations or all the stations for a Line Segment. To edit the data, double-click a line, or click the New button. Related topics Assembly control overview Line station variants and line station orders Line Segment A set of consecutive assembly-line work centers on an assembly line between two buffers. The first buffer is the beginning of the segment, the next buffer is the first part of the next segment. Line Segment A set of consecutive assembly-line work centers on an assembly line between two buffers. The first buffer is the beginning of the segment, the next buffer is the first part of the next segment. Station A line station or a line buffer that is linked to the line segment. Station Type The type of the line station. Next Station The station that comes after the station or buffer defined in the Station field. Only the last line station of the supplying line can be linked to multiple line stations on different parent lines. For more information, refer to Linking a supply line to multiple parent lines (Divergent assembly line structure) Assembly line selection— Configuration Dependent parameter Synchronizing a supply line with mutiple parent lines Transportation time for linked assembly lines Segment of next station The line segment of Next Station. You cannot link a line station to more than one line stations of the same assembly line in the same effective period. You cannot link last line station of an assembly line to more than one line stations of the same segment in the same effective period. If line station is linked to a line station of the same segment or the same assembly line, it is not allowed to link this station to another station in the same effective period. For more information, refer to Linking a supply line to multiple parent lines (Divergent assembly line structure) Assembly line selection— Configuration Dependent parameter Synchronizing a supply line with mutiple parent lines Transportation time for linked assembly lines Effective Date The first date when the line stations in this line are valid. This field cannot be empty. Expiry Date The last date when the line stations in this line are valid. If this field is empty, the stations are always valid. |