| # Preventive Maintenance Scenario Lines (tsspc1131m000) Use this session to create and maintain preventive maintenance scenario lines based on which a maintenance plan is generated for a serialized item. Scenarios can be: Usage Based. Example execute maintenance after 10000 km or after profile of the tire is below 3 mm. Time Based. Example 12 times a year. Based on time according to a predefined pattern. Example perform minor maintenance after two months, extensive maintenance after three months, minor maintenance after five months. Related topics Service inspections and preventive maintenance scenarios Maintenance Scenario The series code of the maintenance scenario. Description The description or name of the code. Line Number The line number of the maintenance scenario. Each line is identified with a unique number generated by LN. By default, LN increases the existing number by a predefined value. However, you can change the value. Description The description or name of the code. Type The type of maintenance scenario line. Allowed values Type Measurement Type The code of the measurement type. Note Only applicable for usage based scenario lines. Description The description or name of the code. Specific Position If this check box is selected, the maintenance scenario line is specific to a position of the item. Note Only applicable for usage based scenario lines. Position The position code of the item. Note only applicable when specific position is selected. Description The description or name of the code. Reference Activity The reference activity from which a planned activity is generated. Description The description or name of the code. Specific Child Item If this check box is selected, the maintenance scenario line is applicable to the specific child item. Child Item The child item for which maintenance plan is generated. During Life Cycle If this check box is selected, planned activities are generated within the defined life cycle of the item. The life cycle can be defined in Items - Service (tsmdm2100m000) session. Cyclic If this check box is selected, planned activities are generated continuously within the specified date range. Frequency The number of times the reference activity is to be carried out. Time(s) Per The unit in which the frequency is expressed. |