| # Pager Data (tsmdm1170m000) Use this session to list and maintain paging device details. Note You send pager messages by means of the Dispatch Control (tssoc2105m009) session. The message layout you select determines the information sent to the employees. In the Service Order Parameters (tssoc0100m000) session, you can specify a location in which LN archives all pager messages you send. You can access this session, only if the Paging Active checkbox in the General Service Parameters (tsmdm0100m000) session is selected. Service Employee The code of the employee who uses the pager. Service Employee The name of the employee who uses the pager. Equipment Type The type of the paging device. Pager The code of the paging device. Number The pager's call number. PIN Number The pager's PIN number. Pager Type The type of messages the pager can receive. Message Layout The code of the pager's message layout. Message Layout The name or description of the message layout. Page Provider The code of the paging provider's system that acts as a gateway to paging vendors and paging networks. Page Provider The code of the page provider, selected from the Business Partners (tccom4500m000) session. Active If this check box is selected, the pager is enabled. If this check box is cleared, the pager is inactive. Note You can only select or clear this check box in the details session. Pager Data Text If this check box is selected, some text with further paging-device details is available. |