| # Printing Bill of Material (Multilevel) Select the items for which you want to print a BOM. After you click Print, you can choose from four different types of bills of material: A BOM with quantities prints BOM data that includes the operation, warehouse, length, width, number of units, inventory unit, and net quantity. A BOM with scrap prints BOM data that includes the revision, effective and expiry dates, scrap percentage and quantity, and extra information. A BOM with manufacturing data prints BOM data that includes the revision, effective and expiry dates, lead-time offset, yield aggregate plan, routing scrap aggregate plan, and whether it is a phantom. A BOM with properties prints BOM data that includes the effective and expiry dates, the effective and expiry change orders, the information whether the component items are a standard configuration, unit effective, linked to CHM or EDM, and so on. For each manufactured item, the printed multilevel bill of material displays components at all levels. Example Manufactured item: 150100 Bicycle Europe
Level | Position | Item | Description
--- | --- | --- | ---
1 | 10 | 150101 | Frame
1 | 20 | 160200 | Wheel
2 | 10 | 200135 | Spoke
2 | 20 | 200100 | Hub
3 | 10 | 210100 | Hub case
3 | 20 | 210110 | Ballbearing
The components at level 2 are used to make the item at level 1. The wheel consists of a hub and spokes. The hub case and ballbearings (level 3) are components of the hub. Use the Print Where-used BOM Components (tibom1412m000) session, to print a summarized multilevel BOM. Use the Print Bill of Material (Single-Level) (tibom1410m000) session, to print a single-level BOM. Related topics Structure of a multilevel BOM Scrap and yield Overview of reference designators Alternative materials in BOMs |