| # Storage Inspection - Inventory History (qmptc3503m000) Use this session to display all previous storage inspections for a specific item. Related topics Storage inspections Item In LN, the raw materials, subassemblies, finished products, and tools that can be purchased, stored, manufactured, sold, and so on. An item can also represent a set of items handled as one kit, or exist in multiple product variants. You can also define nonphysical items, which are not held in inventory but can be used to post costs or to invoice services to customers. The following are examples of nonphysical items: Cost items (for example, electricity) Service items Subcontracting services List items (menus/options) Related topics Using codes Sequence The sequence number identifies the storage inspections for a particular item. A common inspection is done for different parts of inventory. The inventory to be inspected can be assigned to the sequence in the Storage Inspection - Inventory (qmptc2130m000) session. Warehouse The warehouse where the inspection took place. Location The location of the warehouse where the inspection took place. Lot The lot that is inspected. Date The date and time when the inspection took place. Quantity Ordered The quantity for which the inspection is required. Consequently, the result of the inspection order concerns the quality of this quantity. Quantity Destroyed The total quantity destroyed during a destructive test, expressed in the order unit. The quantity destroyed is equal to the sample size of the inspection orders that are tested by means of destructive tests. The quantity destroyed does not have any impact on the accepted or rejected quantities. LN only calculates the quantity that is destroyed according to the test. Note This quantity is automatically updated in the Process Inspection Orders (qmptc1204m000) session. Recommended The quantity to be accepted, as recommended by the Quality package, expressed in the inventory unit. The total of all sample quantities which passed the tests successfully. Note This quantity is automatically updated by use of the Process Inspection Orders (qmptc1204m000) session. Recommended The physical quantity in which an item or good is managed. For example, a quantity of wood can be expressed as a length by using the unit of one meter, or as a volume by using the unit of one cubic meter. Recommended The quantity to be rejected as recommended by the Quality package, expressed in the inventory unit. The total of all sample quantities which do not have the required quality level. Note This quantity is automatically updated by use of the Process Inspection Orders (qmptc1204m000) session. |