| # Combined Freight Order Lines (fmlbd1521m000) Use this session to view the combined freight order lines from which a load plan is created. A combined freight order consists of a number of freight order lines that share the same attributes. Related topics The load building process Plan The load plan for which the combined freight order is created. Combined Freight Order A combined freight order on which the load plan is based. A load plan can be based on one or more combined freight orders. The load building process Freight Order Line The identification number of the freight order on which the combined freight order is based. Freight Order Line The position number of the freight order line that belongs to the freight order on which the combined freight order is based. Item The item on the freight order line that is to be transported. Quantity to be Shipped The quantity of the item to be transported. Quantity to be Shipped The unit used to express the quantity of the item to be transported. Additional Rate Quantity A quantity by unit against which you can define freight rates. You can choose from the units defined in Common. Many freight rates are based on distance and weight. Additional quantities/units enable you to define rates that are based on other units, such as volume, or define rates that are based on combinations of distance, weight, and other units. Example 1 Freight rate by additional quantity/unit: Additional Rate Quantity: 1 pallet, Distance: 1000 km Amount by Distance: 10 Example 2 Freight rates by combinations of units by distance/zone: Weight: 10 kg Additional Rate Quantity: 1 m³ Break Type: Minimum
Distance: | 0 | 100 | 500
Amount by Distance | 10 | 15 | 20
Amount by Weight | 5 | 5 | 10
Amount by Additional Rate Unit | 5 | 5 | 7
In this example, freight rates are based on distance by weight and volume. Shipment SH0001, from Amsterdam to Rotterdam, includes the following details: Distance: 70 km, Weight: 50 kg, Volume: 7 m³ The freight costs for shipment SH0001 are:
     10 * 70 (distance) + 5 * 50 (weight) + 5 * 7 (volume) = 985
Additional Rate Quantity The unit used to express the additional rate quantity by unit. Weight The aggregated weight of the item to be transported. Weight The unit used to express the aggregated weight of the item to be transported. Pieces The aggregated piece unit quantity of the item to be transported. Related topics Piece units used in load building and loading capacity checks Piece Unit The piece unit for the items. Related topics Piece units used in load building and loading capacity checks |