| # Preventive Maintenance Scenario Line Patterns (tsspc1132m000) Use this session to create and maintain patterns based on which planned activities are generated. Related topics Service inspections and preventive maintenance scenarios Maintenance Scenario The series code that identifies the maintenance scenario. Description The description or name of the code. Line The maintenance scenario line number. Sequence Number The sequence allows multiple pattern lines under the same scenario line. Reference Activity The reference activity from which a planned activity is to be generated. Description The description or name of the code. Activity Type The activity pattern can be generated either for reference activity or master routing. Master Routing The master routing for which the pattern is generated. Year Number The number of year(s) after which the reference activity is performed. Months/ Weeks The number of month(s) or week(s) after or in-which the reference activity is performed. Month/Week The option to specify when the reference activity must be performed. Allowed values Month or Week Days The number of day(s) after or on which the reference activity will be carried out. Time Period The number of month(s)/week(s) and day(s) after which the reference activity is performed. Overrule Planned Start/Finish Tolerance If this check box is selected, Infor LN does not consider the tolerance period. Tolerance Period Start The maximum time period with which the start date of the generated planned activity can be shifted. Unit for Tolerance Period The unit in which tolerance period is expressed. Tolerance Period Finish The maximum time period with which the finish date of the generated planned activity can be shifted. Specific Child Item If this check box is selected, you can specify the child item. Child Item The child item for which maintenance plan is generated. Description The description or name of the code. |