| # Transportation time between linked assembly lines New in Infor LN 10 In Infor LN 10, a supply line linked to multiple parent lines, can be physically present in the same geographical location as the parent lines, or can be located in a different geographical area. If the supply line is located in a different geographical area, the time to transport assembled components to the parent line must be taken into account when planning the assembly orders. In Infor LN 10 tranportation time is calculated based on these data: Address of the line station on the supply line. Address of the line station on the parent line. For more information, refer to Transportation time for linked assembly lines. Related topics Linking a supply line to multiple parent lines (Divergent assembly line structure) Synchronizing a supply line with mutiple parent lines Assembly line selection— Configuration Dependent parameter |