| # Freight Order Control Parameters (fmfoc0100m000) Use this session to maintain the Freight Order Control parameters. In this session, you can define the following settings: Number group for freight orders. Series for freight orders originating from warehouse, sales, purchase, or enterprise planning orders. Default values for freight orders such as transport types. Default loading and unloading date tolerances for freight orders that originate from purchase orders, sales orders, enterprise planning orders, and warehouse orders. Related topics Load and unload date/time tolerances Effective Date effective date. In the actual set, or parameter set, the Effective Date field is empty, but the effective date is taken as the default value in the Description field. In parameter sets that precede the actual set, the effective date is displayed in the Effective Date field. If you make a change in the actual set, the changed set becomes the new actual set. Number Group for Freight Orders The number group that is to be used for freight orders. Step Size for Freight Order Lines In this field you can define the interval for freight order line numbers, for example 10, 20, 30, or 5, 10, 15. Therefore, the first freight order line receives number 10, the second number 20, and the third receives number 30, or the first freight order line receives number 5, the second receives number 10, and the third number 15. Transport Type The default transport type that is added to new freight orders. If a transport means combination or a transport means group is selected for the current parameter set, the transport type is taken from the transport means combination or transport means group. You must not change this value. Related topics The use of transport types Multiple means of transport by load Transport Means Group The default transport means group for freight orders. For the transport means group that you select in this field, the Independent Use Allowed check box must be selected. Related topics The use of transport means groups Multiple means of transport by load Transport Means Combination The default Transport means combination for freight orders. If a transport means group is selected in the Transport Means Group field, you cannot select a transport means combination. If a carrier is inserted for the current item, the transport means combination must be attached to this carrier. In the Transport Means Combinations by Carrier (fmfmd0144m000) session, you can attach transport means combinations to carriers. Related topics Multiple means of transport by load The use of transport means groups Series for Purchase Origin The series to be used for freight orders originating from purchase orders. Series for Sales Origin The series to be used for freight orders originating from sales orders. Series for Warehouse Origin The series to be used for freight orders originating from warehouse orders. Freight Order Type The default freight order type that is added to new freight orders. Related topics The use of freight order types Engineering Revisions Active If this check box is selected, engineering item revision control is active. Engineering item revisions are defined in Manufacturing. An item can have several revisions. Revision codes are derived from the revised engineering items. Series for EP Origin The series to be used for freight orders originating from Enterprise Planning orders. Series for Service and Maintenance Origin The series to be used for freight orders originating from Service orders. Log Freight Order History If this check box is selected, a history record is created for each change that is made to a freight order or a freight order line. If you do not require history records for freight orders or freight order lines, clear this check box. Performance aspects The setting of this field could affect system performance and database growth. For more information, refer to History data. Earliest Load Date Tolerance The time limit prior to a freight order's planned load date/time by which you can exceed the planned load date/time. The time limit is expressed in user definable time units. Related topics Load and unload date/time tolerances Lead time calculations for originating orders Earliest Load Date Tolerance The time unit used to express the tolerance. Latest Load Date Tolerance The time limit following a freight order's planned load date/time by which you can exceed the planned load date/time. The time limit is expressed in user-definable time units. Related topics Load and unload date/time tolerances Lead time calculations for originating orders Earliest Unload Date Tolerance The time limit prior to a freight order's planned unload date/time that you can exceed the planned unload date/time. The time limit is expressed in user-definable time units. Related topics Load and unload date/time tolerances Lead time calculations for originating orders Earliest Unload Date Tolerance The time unit used to express the tolerance. Latest Unload Date Tolerance The time limit following a freight order's planned unload date/time that you can exceed the planned unload date/time. The time limit is expressed in user-definable time units. Related topics Load and unload date/time tolerances Lead time calculations for originating orders Earliest Load Date Tolerance The time limit prior to a freight order's planned load date/time by which you can exceed the planned load date/time. The time limit is expressed in user definable time units. Related topics Load and unload date/time tolerances Lead time calculations for originating orders Earliest Load Date Tolerance The time unit used to express the tolerance. Latest Load Date Tolerance The time limit following a freight order's planned load date/time by which you can exceed the planned load date/time. The time limit is expressed in user-definable time units. Related topics Load and unload date/time tolerances Lead time calculations for originating orders Earliest Unload Date Tolerance The time limit prior to a freight order's planned unload date/time that you can exceed the planned unload date/time. The time limit is expressed in user-definable time units. Related topics Load and unload date/time tolerances Lead time calculations for originating orders Earliest Unload Date Tolerance The time unit used to express the tolerance. Latest Unload Date Tolerance The time limit following a freight order's planned unload date/time that you can exceed the planned unload date/time. The time limit is expressed in user-definable time units. Related topics Load and unload date/time tolerances Lead time calculations for originating orders Earliest Load Date Tolerance The time limit prior to a freight order's planned load date/time by which you can exceed the planned load date/time. The time limit is expressed in user definable time units. Related topics Load and unload date/time tolerances Lead time calculations for originating orders Earliest Load Date Tolerance The time unit used to express the tolerance. Latest Load Date Tolerance The time limit following a freight order's planned load date/time by which you can exceed the planned load date/time. The time limit is expressed in user-definable time units. Related topics Load and unload date/time tolerances Lead time calculations for originating orders Earliest Unload Date Tolerance The time limit prior to a freight order's planned unload date/time that you can exceed the planned unload date/time. The time limit is expressed in user-definable time units. Related topics Load and unload date/time tolerances Lead time calculations for originating orders Earliest Unload Date Tolerance The time unit used to express the tolerance. Latest Unload Date Tolerance The time limit following a freight order's planned unload date/time that you can exceed the planned unload date/time. The time limit is expressed in user-definable time units. Related topics Load and unload date/time tolerances Lead time calculations for originating orders Earliest Load Date Tolerance The time unit used to express the tolerance. Earliest Load Date Tolerance The time unit used to express the tolerance. Earliest Load Date Tolerance The time limit prior to a freight order's planned load date/time by which you can exceed the planned load date/time. The time limit is expressed in user definable time units. Related topics Load and unload date/time tolerances Lead time calculations for originating orders Earliest Load Date Tolerance The time limit prior to a freight order's planned load date/time by which you can exceed the planned load date/time. The time limit is expressed in user definable time units. Related topics Load and unload date/time tolerances Lead time calculations for originating orders Latest Load Date Tolerance The time limit following a freight order's planned load date/time by which you can exceed the planned load date/time. The time limit is expressed in user-definable time units. Related topics Load and unload date/time tolerances Lead time calculations for originating orders Latest Load Date Tolerance The time limit following a freight order's planned load date/time by which you can exceed the planned load date/time. The time limit is expressed in user-definable time units. Related topics Load and unload date/time tolerances Lead time calculations for originating orders Earliest Unload Date Tolerance The time unit used to express the tolerance. Earliest Unload Date Tolerance The time limit prior to a freight order's planned unload date/time that you can exceed the planned unload date/time. The time limit is expressed in user-definable time units. Related topics Load and unload date/time tolerances Lead time calculations for originating orders Earliest Unload Date Tolerance The time limit prior to a freight order's planned unload date/time that you can exceed the planned unload date/time. The time limit is expressed in user-definable time units. Related topics Load and unload date/time tolerances Lead time calculations for originating orders Latest Unload Date Tolerance The time limit following a freight order's planned unload date/time that you can exceed the planned unload date/time. The time limit is expressed in user-definable time units. Related topics Load and unload date/time tolerances Lead time calculations for originating orders Latest Unload Date Tolerance The time limit following a freight order's planned unload date/time that you can exceed the planned unload date/time. The time limit is expressed in user-definable time units. Related topics Load and unload date/time tolerances Lead time calculations for originating orders Loading during calendar time-window If this check box is selected, you can load on the planned load date during the opening hours of the loading address, as specified in the calendar of the loading address. If this check box is cleared, you can load on the planned load date and time, including the load date tolerances defined in the current session or the Addresses - Freight Management (fmfmd0110m000) session. If you want this setting to apply to all loading addresses, select this check box in the current session. If you want this setting to apply to individual loading addresses, select this setting for the required addresses in the Addresses - Freight Management (fmfmd0110m000) session. Example The loading address is open between 06:00 and 20:00 on the planned load date. The planned time is 17:00 and the load date tolerance of the address is four hours. If you do not select this check box, the earliest time would be 13:00, and the latest time would be next day at 07:00. If you select the check box, the earliest time would be 06:00 and the latest time would be 20:00 on the same day. Related topics Load and unload date/time tolerances Loading during calendar time-window If this check box is selected, you can load on the planned load date during the opening hours of the loading address, as specified in the calendar of the loading address. If this check box is cleared, you can load on the planned load date and time, including the load date tolerances defined in the current session or the Addresses - Freight Management (fmfmd0110m000) session. If you want this setting to apply to all loading addresses, select this check box in the current session. If you want this setting to apply to individual loading addresses, select this setting for the required addresses in the Addresses - Freight Management (fmfmd0110m000) session. Example The loading address is open between 06:00 and 20:00 on the planned load date. The planned time is 17:00 and the load date tolerance of the address is four hours. If you do not select this check box, the earliest time would be 13:00, and the latest time would be next day at 07:00. If you select the check box, the earliest time would be 06:00 and the latest time would be 20:00 on the same day. Related topics Load and unload date/time tolerances Unloading During Calendar Time Window If this check box is selected, you can unload on the planned unload date during the opening hours of the unloading address, as specified in the calendar of the unloading address. If this check box is cleared, you can unload on the planned unload date and time, including the unload date tolerances. If you want this setting to apply to all unloading addresses, select this check box in the current session. If you want this setting to apply to individual unloading addresses, select this setting for the required addresses in the Addresses - Freight Management (fmfmd0110m000) session. Example The unloading address is open between 06:00 and 20:00 on the planned unload date. The planned time is 17:00 and the unload date tolerance of the address is four hours. If you do not select this check box, the earliest time would be 13:00, and the latest time would be next day at 07:00. If you select the check box, the earliest time would be 06:00 and the latest time would be 20:00 on the same day. Related topics Load and unload date/time tolerances Unloading During Calendar Time Window If this check box is selected, you can unload on the planned unload date during the opening hours of the unloading address, as specified in the calendar of the unloading address. If this check box is cleared, you can unload on the planned unload date and time, including the unload date tolerances. If you want this setting to apply to all unloading addresses, select this check box in the current session. If you want this setting to apply to individual unloading addresses, select this setting for the required addresses in the Addresses - Freight Management (fmfmd0110m000) session. Example The unloading address is open between 06:00 and 20:00 on the planned unload date. The planned time is 17:00 and the unload date tolerance of the address is four hours. If you do not select this check box, the earliest time would be 13:00, and the latest time would be next day at 07:00. If you select the check box, the earliest time would be 06:00 and the latest time would be 20:00 on the same day. Related topics Load and unload date/time tolerances Loading during calendar time-window If this check box is selected, you can load on the planned load date during the opening hours of the ship-from address, as specified in the Calendar of the loading address. If this check box is cleared, you can load on the planned load date and time, as specified in the load date tolerances. If you want this setting to apply to all loading addresses, select this check box in the current session. If you want this setting to apply to individual loading addresses, select this setting for the required addresses in the Addresses - Freight Management (fmfmd0110m000) session. Example The loading address is open between 06:00 and 20:00 on the planned load date. The planned time is 17:00 and the load date tolerance of the address is four hours. If you do not select this check box, the earliest time would be 13:00, and the latest time would be next day at 07:00. If you select the check box, the earliest time would be 06:00 and the latest time would be 20:00 on the same day. Related topics Calendar time-windows Load and unload date/time tolerances To define loading and unloading date/time tolerances Unloading During Calendar Time Window If this check box is selected, you can unload on the planned unload date during the opening hours of the unloading address, as specified in the calendar of the unloading address. If this check box is cleared, you can unload on the planned unload date and time, including the unload date tolerances. If you want this setting to apply to all unloading addresses, select this check box in the current session. If you want this setting to apply to individual unloading addresses, select this setting for the required addresses in the Addresses - Freight Management (fmfmd0110m000) session. Example The unloading address is open between 06:00 and 20:00 on the planned unload date. The planned time is 17:00 and the unload date tolerance of the address is four hours. If you do not select this check box, the earliest time would be 13:00, and the latest time would be next day at 07:00. If you select the check box, the earliest time would be 06:00 and the latest time would be 20:00 on the same day. Related topics Load and unload date/time tolerances Loading during calendar time-window If this check box is selected, you can load on the planned load date during the opening hours of the loading address, as specified in the calendar of the loading address. If this check box is cleared, you can load on the planned load date and time, including the load date tolerances. If you want this setting to apply to all loading addresses, select this check box in the current session. If you want this setting to apply to individual loading addresses, select this setting for the required addresses in the Addresses - Freight Management (fmfmd0110m000) session. Example The loading address is open between 06:00 and 20:00 on the planned load date. The planned time is 17:00 and the load date tolerance of the address is four hours. If you do not select this check box, the earliest time would be 13:00, and the latest time would be next day at 07:00. If you select the check box, the earliest time would be 06:00 and the latest time would be 20:00 on the same day. Related topics Load and unload date/time tolerances Unloading During Calendar Time Window If this check box is selected, you can unload on the planned unload date during the opening hours of the unloading address, as specified in the calendar of the unloading address. If this check box is cleared, you can unload on the planned unload date and time, including the unload date tolerances. If you want this setting to apply to all unloading addresses, select this check box in the current session. If you want this setting to apply to individual unloading addresses, select this setting for the required addresses in the Addresses - Freight Management (fmfmd0110m000) session. Example The unloading address is open between 06:00 and 20:00 on the planned unload date. The planned time is 17:00 and the unload date tolerance of the address is four hours. If you do not select this check box, the earliest time would be 13:00, and the latest time would be next day at 07:00. If you select the check box, the earliest time would be 06:00 and the latest time would be 20:00 on the same day. Related topics Load and unload date/time tolerances Loading during calendar time-window If this check box is selected, you can load on the planned load date during the opening hours of the loading address, as specified in the calendar of the loading address. If this check box is cleared, loading is possible on the planned load date and time, including the load date tolerances. If you want this setting to apply to all loading addresses, select this check box in the current session. If you want this setting to apply to individual loading addresses, select this setting for the required addresses in the Addresses - Freight Management (fmfmd0110m000) session. Example The loading address is open between 6:00 and 20:00 on the planned load date. The planned time is 17:00 and the load date tolerance of the address is four hours. If you do not select this check box, the earliest time would be 13:00, and the latest time would be next day at 07:00. If you select the check box, the earliest time would be 06:00 and the latest time would be 20:00 on the same day. Related topics Load and unload date/time tolerances Unloading During Calendar Time Window If this check box is selected, you can unload on the planned unload date during the opening hours of the unloading address, as specified in the calendar of the unloading address. If this check box is cleared, you can unload on the planned unload date and time, including the unload date tolerances. If you want this setting to apply to all unloading addresses, select this check box in the current session. If you want this setting to apply to individual unloading addresses, select this setting for the required addresses in the Addresses - Freight Management (fmfmd0110m000) session. Example The unloading address is open between 06:00 and 20:00 on the planned unload date. The planned time is 17:00 and the unload date tolerance of the address is four hours. If you do not select this check box, the earliest time would be 13:00, and the latest time would be next day at 07:00. If you select the check box, the earliest time would be 06:00 and the latest time would be 20:00 on the same day. Related topics Load and unload date/time tolerances Carrier The default Carrier for freight orders. Series for Manual Freight Orders The series to be used for manually created freight orders. Number Group Freight Order Clusters The number group that is to be used for freight order clusters. Series for Freight Order Clusters The series to be used for freight order clusters. Series for Freight Order Clusters The description of the series to be used for freight order clusters. Series for Warehousing Clusters The series to be used for freight order clusters generated by Warehousing. Series for Directly Delivered Clusters The series to be used for directly delivered freight order clusters. Step Size for Freight Order Cluster Lines In this field you can define the interval for freight order cluster line numbers, for example 10, 20, 30, or 5, 10, 15. Therefore, the first freight order cluster line receives number 10, the second number 20, and the third receives number 30, or the first freight order cluster line receives number 5, the second receives number 10, and the third number 15. Step Size for Additional Cost Lines The interval for additional cost line numbers, for example, 10, 20, 30, or 5, 10, 15. First Line for Additional Cost Lines The first position number for cluster lines that contain additional costs. Log Freight Order Cluster History If this check box is selected, a history record is created for each change that is made to a freight order cluster or a freight order cluster line. If you do not require history records for freight orders or freight order lines, clear this check box. Performance aspects The setting of this field could affect system performance and database growth. For more information, refer to History data. Waiting Time for Loading The time spent waiting until loading can take place. The lead times defined in this session are used as default lead times in load building for addresses that have not been defined in the Addresses - Freight Management (fmfmd0110m000) session. Time for Loading The time required for loading. The lead times defined in this session are used as default lead times in load building for addresses that have not been defined in the Addresses - Freight Management (fmfmd0110m000) session. Waiting Time for Unloading The time spent waiting until unloading can take place. The lead times defined in this session are used as default lead times in load building for addresses that have not been defined in the Addresses - Freight Management (fmfmd0110m000) session. Time for Unloading The time required for unloading. The lead times defined in this session are used as default lead times in load building for addresses that have not been defined in the Addresses - Freight Management (fmfmd0110m000) session. |