| # Test Data History by Characteristic (qmptc3515m000) Use this session to display the test data history by characteristic. The data was previously entered in the Sample - Test Data by Characteristic (qmptc1115m000) details session. Test data lines were generated based on the test quantity (see the Inspection Order - Samples (qmptc1110m000) session). Example
Sample quantity | 100 pieces
Test quantity | 20 pieces
Explanation: You must do five tests on twenty pieces to get a sample quantity of one hundred pieces (100/20=5). Consequently, five test lines are generated. Related topics Order inspections Inspection Order The code of the inspection order. Sample A small quantity that is drawn from the total (order) quantity and which represents the order quantity's quality. Line The position number represents a characteristic that is measured. The measured value is entered as test data in the Sample - Test Data by Characteristic (qmptc1115m000) session. Characteristic A reference to a particular quality or distinctive mark of an item or an item part/component. For example, diameter, length, weight. Characteristic Type The type of value that is measured. Item In LN, the raw materials, subassemblies, finished products, and tools that can be purchased, stored, manufactured, sold, and so on. An item can also represent a set of items handled as one kit, or exist in multiple product variants. You can also define nonphysical items, which are not held in inventory but can be used to post costs or to invoice services to customers. The following are examples of nonphysical items: Cost items (for example, electricity) Service items Subcontracting services List items (menus/options) Serial Number A unique number that Infor LN generates to distinguish between the different measurements that you can do in one sample quantity. The number of measurements is based on the test quantity.
Example
Sample quantity | 100 pieces
Test quantity | 20 pieces
Explanation: You must do five tests on twenty pieces to get a sample quantity of one hundred pieces (100/20=5). Consequently, five test lines are generated, with each an unique serial number. Note The total number of serial numbers cannot exceed the value of the sample quantity divided by the test quantity Test Date The date and time when the test took place. Measurement Value The result of the test. A numeric value is displayed if you select Quantitative in the Result Type field, and if the Characteristic Type field is not set to Option. If an algorithm is specified for the inspection order line, the algorithm calculated the numeric value that is displayed in this field. Unit The unit in which the test results are defined or calculated. Note This field does not apply if you enter Option in the Characteristic Type field. Option Set The name of the option set. Option The option that was found. Note Depending on what you entered in the Option Type field in the Option Set - Options (qmptc0114m000) session, the option is either Acceptable or Not Acceptable. Result The result of the inspection. Note LN automatically generates a value, depending on the quality limits that you defined in the Characteristics (qmptc0115m000) session and/or in the Option Set - Options (qmptc0114m000) session. Test Area The physical location where tests take place. Employee The person that performs the test on this characteristic. Instrument The default instrument used to measure the characteristic. Description The description or name of the code. Instrument Number The number of the instrument that can be used to trace the instrument. |