| # Production order planning of generic items The generic routing, defined in the Generic Item - Structure (tipcf3100m100) session, differs from the normal routing. Which operations are used in the routing, depends on the configuration. Example Two operations might be exclusive: either operation 10 is selected, or operation 20. As a result, a sequence of operations is not required. Therefore, the operation of a generic routing has several parameters for planning: Planned Production Time Planning Percentage Lead Time Offset For the lead time, the planning percentage is taken into account.
    Operation lead time = planned production time * planning percentage
The lead time offset is used to determine the start of the operation sequence. Planned production order for generic item Related topics Calendars in Enterprise Planning Horizons and time fences Time Zones in Enterprise Planning |