| # Maintenance Triggers (tsmdm0169m100) Use this session to define alphanumeric maintenance triggers for the maintenance trigger set. Note When you perform an inspection, LN checks for an applicable maintenance trigger set. If the measured value meets with one of the maintenance triggers within the trigger set, a maintenance notification is generated. Related topics Service inspections and preventive maintenance scenarios Maintenance Trigger Set The maintenance triggers set to which the trigger belongs. Description The description or name of the code. Trigger Number The unique ID of the maintenance trigger. Value is The value of the alphanumeric trigger that triggers the creation of a maintenance notification. Alphanumeric measurement values defined for the measurement type of the maintenance trigger set are listed. Trigger Message The code of the trigger message. For alphanumeric measurement values LN defaults the Trigger Message from the Alphanumeric Measurement Values (tsmdm0166m000) session. Description The description or name of the code. Default Recommendation The recommendation defined as the default value for the maintenance trigger. LN defaults the value only if the Default check box is selected in the Recommendation (tsmdm0167m000) session. Recommendation The description or name of the code. Default Follow-up Activity The reference activity defined as the default value for the maintenance trigger. Description The description or name of the code. |