| # Sampling Rules (qmptc0160m000) Use this session to define sampling rule that are used for a standard test procedure. Sampling Rule The unique code of the sampling rule. Description The description or name of the code. Sampling Plan The unique code of the sampling plan. Description The description or name of the code. General Code Letter Table The unique code of the code letter table. Description The description or name of the code. Inspection Level The inspection level that must be executed. Description The description or name of the code. Inspection Standard The unique code of the inspection standard. Description The description or name of the code. Skip Lot If this check box is selected, only a part of the submitted lot is to be inspected. Skip Frequency The number of lots (or batches) that can be skipped for inspection. Decreased Inspection Accepted Consecutive Batches The number of accepted batches that are required for switching to a less inspection procedure. When goods are supplied with steady quality, a switch can be made to a decreased/less inspection procedure. Sampling Rule The code of the sampling rule used for the decreased/looser inspection regime. Description The description or name of the code. Increased Inspection Rejected Batches The number of rejected batches that trigger the shift to a tighter inspection regime. Batch Horizon The number of most recent, consecutive batches that must be checked to trigger a tighter inspection regime. Sampling Rule The sampling rule to be used for the increased/tighter inspection regime. Description The description or name of the code. Print Sampling Rules Prints the sampling rules. |