| Address Types by Service (ttcmf0140m000) |  |
| use.session.to set up the link between an address type and its type of service. You can also specify whether you want the user to be able to preview a message of this type of service. Follow this procedure to enter a new address type: Enter an address type and description. Select the UI Required check box if you want the user to be able to make changes before the message transfer is complete. Enter the name of the service. Each service can have more than one address type, which means that a service can appear on this list more than once.
Fields | Description
Address Type | Enter a valid eMessage Connector address type, such as SMTP, FAX, Telex, SITA, or SMS. To see the valid address types, see the domain ttcmf.type in version 0a.
UI Required | If this check box is selected, additional user interaction is allowed before the message transfer is complete. For example, the Outlook connector allows user interaction.
Resolve Capability | If this check box is selected, the service shown in Service Name has the capability to resolve an address when given a name and address type. Currently only the Outlook connector supports this.
Service Name | Enter a service from the Services (ttcmf0130m000) session. Click on the right arrow to display a list of valid services. Each service can have more than one address type.
Service Name | The description of the service.
Paper Type | Choose the paper type.