| Possible Values |  |
| Continuous Sampling This type of sampling only takes place in case of mass production and is used to control processing. After a particular interval, a sample is drawn equally large as the sample size. A decision is taken based on the quality of the sample whether to continue the production or to stop and take corrective action. For this test type, data must be entered in the following fields: - Frequency Unit - Quantity 100 All items are inspected. The sample size and the order quantity have the same value. Single Sampling One sample out of the entire order quantity is inspected. |