| Validate Assembly Lines (tiasl1230m000) |  |
| Use this session to validate that assembly lines and assembly line structures are correctly defined. Before you can actualize a line structure, you must validate it. Note You can run this session only in the master company. If errors are detected in the assembly line (structure), an error report is printed and the status of the assembly line(s) is set to Modified. Alternatively, to validate a line structure, you can run the Actualize Assembly Lines (tiasl1231m000) session. This session validates the line structure and then starts the actualization process.
Fields | Description
Assembly Line | The range of assembly lines to validate.
Commands | Description
Validate | Starts validating.