| Process EBOM Changes (tiedm3205m000) |  |
| Use this session to generate single-level EBOMs for the revisions which have been generated or modified by MBCs. The single-level EBOMs are based on the E-items from the E-Item by MBC (tiedm3122m000) session and on the order lines from the MBC Action (tiedm3120m000) session. Limits to the use of this session Engineering BOMs can only be modified with this session if the following applies: The order status is Approved by Engineering. E-items have been generated using the Generate E-Items by MBC (tiedm3201m000) session, or modified with the E-Item by MBC (tiedm3122m000) session for the current MBC. Revisions Changes resulting from MBCs are based on the most recent revision. If that revision is: Linked to an order, the MBC order status must be Approved by Engineering. Not linked to an MBC but is manually defined in the Engineering Item Revision (tiedm1100m000) session, EBOM lines must be present in the Engineering BOM (tiedm1110m000) session for that revision. Different from the revision in the Old Revision field in the E-Item by MBC (tiedm3122m000) session, Old Revision will be overwritten with the revision on which the change is based. Processing EBOM changes Single-level EBOMs are changed in two steps: The old revision of the E-item of the EBOM is copied to the new revision. (See the Old Revision field and New Revision field in the E-Item by MBC (tiedm3122m000) session.) The actions that you have indicated in the MBC Action (tiedm3120m000) session are performed on the new EBOM. After you change the EBOMs, ERP LN carries out the following actions: The order status becomes Approved by Production. The revisions generated by the MBC are automatically released (or manually released, in the Engineering Item Revision (tiedm1100m000) session). Automatic releasing is not possible for an E-item which has no relationship with items. If applicable the Number of Units, Length, Width and Net Quantity fields in the Engineering BOM (tiedm1110m000) session are filled. Related topics Calculating net quantity Engineering data management summary To change EBOMs - Automatic procedure Finalizing engineering data
Fields | Description
MBC Number | Enter a range of MBCs, whose changes to EBOMs you want to process. Related topics To use From and To fields
MBC Number | Enter a range of MBCs, whose changes to EBOMs you want to process. Related topics To use From and To fields
Approve New Revisions by Engineering | If this check box is selected, the status of new revisions is automatically set to Approved by Engineering after their EBOMs have been generated. If this check box is cleared, you must approve revisions using the Engineering Item Revision (tiedm1100m000) session.