| Calculating production rate and cycle time from a norm table |  |
| Production rate The production rate is the number of norm units per minute or per hour that a task can be performed for a combination of an X-axis value and a Y-axis value from the norm table, multiplied by a conversion factor. This conversion factor is defined for the norm table in the Norm Tables (tirou0130m000) session. Note If you have selected a value that does not appear on the X-axis or the Y-axis, the production rate will be calculated by linear interpolation. For more information, see Calculating based on norm tables. Example 1 (norm units in MINUTES)
Norm table code | AAA Sawing boards
Conversion factor | 1.0000
Board width in mm | Board diameter in mm | 50.00 | 70.00 | 90.00
4.00 | - | 7 | 6 | 5
6.00 | - | 5 | 4 | 3
8.00 | - | 3 | 2 | 1
If a board has a width of 60.00 mm and a thickness of 4 mm, seven boards can be sawn per minute if the conversion factor is 1.0000. If you change the conversion factor to 10.0000, 60 boards can be sawn per minute. The values in the table remain unchanged, whatever the value of the conversion factor. The result of a change is not visible until the computation of the norm time and the production rate (norm units) on the Calculated Norm Time field and the Calculated Production Rate field in the Calculate Norm Time (tirou0230m000) session. The number of units is per minute or per hour, depending on the value of the Production Rate Time Unit field in the Routing Parameters (tirou0100m000) session. Cycle time The cycle time is the required norm time in MINUTES to perform an operation on one piece of an item for a combination of the norm table's X-axis value and a Y-axix value multiplied by two conversion factors. These factors are defined in the Conversion Factor Norm Times field in the Norm Tables (tirou0130m000) session and Factor for Norm Time field in the Calculate Norm Time (tirou0230m000) session. Note If you have selected a value that does not appear on the X-axis or Y-axis, the cycle time will be calculated by interpolation. Example 2 (norm times in MINUTES)
Norm table | 10B Drilling holes
Conversion factor | 1.0000
Board thickness in mm | Hole thickness in mm | 5.00 | 7.00 | 9.00
40 | - | 0.500 | 1.000 | 1.500
50 | - | 1.000 | 1.500 | 2.000
75 | - | 2.000 | 2.500 | 3.000
If the conversion factor is 1.0000, it takes a half a minute to drill a hole with a diameter of 5 mm in a board with a thickness of 40 mm. If you change the conversion factor to 10.000, it will take 5 minutes to drill the hole. The values in the table remain unchanged, irrespective of the value of the conversion factor. The result of a change is not visible until the computation and the production rate (norm units) is done on the calculated norm time fields and calculated production rate fields in the Calculate Norm Time (tirou0230m000) session. Related topics Calculating based on norm tables |