| Product Variant Structures (tiapl3510m000) |  |
| Use this session to view and maintain product variant structures. A product variant structure defines the structure of a specific configured item by specifying the relations between this item and the generic items and engineering modules that make up this item. Generic sub-items can also have their own sub-items and/or engineering modules. The level below the engineering modules is specified in the flattened assembly parts, which appears in the Assembly BOM and Operations (tiapl2520m000) session. The product variant structure is created on the following moments: When the product variant is entered and saved, the product variant structure is created, in regard to the relation between the main item and the generic sub items. When you run the Generate Product Variant Structures (tiapl3210m000) ) session, the product variant structure is created, in regard to the relation between the main item and the engineering modules. Note, however, that this only happens if the External Product Variant Structure check box is cleared in the details of the Assembly Planning Parameters (tiapl0500m000) session. If required, the product variant structure can also be generated by the following sessions: Generate Assembly Orders (tiapl3201m000) Refresh and Freeze Assembly Orders (tiapl3203m000) The generic items and engineering modules are retrieved from the following sources: The bill of material (BOM) relations to generic sub items are always copied from the item's template, which is defined in the Generic Bill of Material (tiapl2510m000) session. The BOM relations to engineering modules are either copied from the item's template, or delivered by an external source, which depends on the selection of the External Product Variant Structure check box in the Assembly Planning Parameters (tiapl0500m000) session. If this check box is selected, the BOM relations to engineering modules are delivered from an external source. ERP LN provides no functionality to copy the engineering modules from an external source to the product variant structure. If this check box is cleared, the BOM relations to engineering modules are copied from the item's template, which is defined in the Generic Bill of Material (tiapl2510m000) session. The information that is retrieved from the generic BOM is selected, based on the effectivity unit of the product variant, and the effective and expiry dates. The date range is evaluated against the Product Configuration Date, which is displayed in the details of the Product Variants (tiapl3500m000) session. You can only change the data in the current session if the following conditions apply: Your current company is defined as master company in the Assembly Planning Parameters (tiapl0500m000) session. You work in Test Mode, which is also defined in the Assembly Planning Parameters (tiapl0500m000) session. The Assembly Status, which appears in the Product Variants (tiapl3500m000) session, is Open. Product variant structures are deleted if the corresponding product variants are deleted. Refer to the To Be Deleted check box in the details of the Product Variants (tiapl3500m000) session, and to the Purge Product Variants (tiapl3200m000) session for more information. You can also generate product variant structures for configurable items. You can use a configurable item to create a item structure that can hold a configurable purchased sub-assembly. For more information on procuring purchased configurable items in Assembly Control module, refer to Procuring configured items in Assembly Control - Master Data Setup Procuring configured items in Assembly Control - BOM setup Product variants - Purchased configurable items Related topics Assembly planning overview
Fields | Description
Product Variant | The code of the product variant for which the product variant structure is displayed.
Main Item | The generic item or manufactured item for which the Default Supply Source is Assembly. This item can be the end item, or a generic item between the end item and the engineering modules. The item must have the following characteristics: The item type must be Generic or manufactured for which the Default Supply Source is Assembly. The item must be Serialized The item must have ordering data The item ordering system must be FAS These characteristics are defined in the Items - General (tcibd0501m000) session and the Items - Ordering (tcibd2500m000) session.
Assembly Line | The assembly line that manufactures the product variant. For more information, refer to Linking a supply line to multiple parent lines (Divergent assembly line structure) Assembly line selection - The Configuration Dependent parameter Synchronizing a supply line with mutiple parent lines Transportation time for linked assembly lines
Position Number | The component's position number that identifies the combination of the main item and the sub item. By default, ERP LN shows the last position number used, plus 10. This procedure provides the sequence 10, 20, 30, and so on. The numbering of positions is unrestricted. It is recommended to use the default values so that you can use intermediate numbers to insert components.
Item | The generic item or engineering module that is directly below the level of the displayed main item in the product variant structure.
Item Type | The item type of the sub item. The item type is either Generic or Engineering Module.
Option Set | Identifies a set with product features and options for a configurable item within the product structure. Related topics Linking a supply line to multiple parent lines (Divergent assembly line structure) Assembly line selection - The Configuration Dependent parameter Synchronizing a supply line with mutiple parent lines Transportation time for linked assembly lines
Assembly Line Location | The physical location of the assembly line. For more information, refer to Linking a supply line to multiple parent lines (Divergent assembly line structure) Assembly line selection - The Configuration Dependent parameter Synchronizing a supply line with mutiple parent lines Transportation time for linked assembly lines
Line Segment Location | The physical location of the line segment. For more information, refer to Linking a supply line to multiple parent lines (Divergent assembly line structure) Assembly line selection - The Configuration Dependent parameter Synchronizing a supply line with mutiple parent lines Transportation time for linked assembly lines
Line Station Location | The physical location of the line station. For more information, refer to Linking a supply line to multiple parent lines (Divergent assembly line structure) Assembly line selection - The Configuration Dependent parameter Synchronizing a supply line with mutiple parent lines Transportation time for linked assembly lines
Operation | One of a series of steps in a routing that are carried out successively to produce an item. The following data is collected during a routing operation: The task. For example, sawing. The machine used to carry out the task (optional). For example, sawing machine. The place where the task is carried out (work center). For example, woodwork. The number of employees required to carry out the task. This data is used to compute order lead times, to plan production orders and to calculate cost prices. Related topics Linking a supply line to multiple parent lines (Divergent assembly line structure) Assembly line selection - The Configuration Dependent parameter Synchronizing a supply line with mutiple parent lines Transportation time for linked assembly lines
Net Quantity | The quantity of a component or material that is theoretically required to make a certain quantity of a product. This quantity is referred to as the net quantity because in practice you may need more than this quantity to make up for certain losses of the material or the product. Related topics Linking a supply line to multiple parent lines (Divergent assembly line structure) Assembly line selection - The Configuration Dependent parameter Synchronizing a supply line with mutiple parent lines Transportation time for linked assembly lines
Commands | Description
Generate Product Variant Structures | Starts the Generate Product Variant Structures (tiapl3210m000) session.
Assembly BOM and Operations | Starts the Assembly BOM and Operations (tiapl2520m000) session.
Where-used Engineering Modules | Starts the Where-used Engineering Modules (tiapl3511m000) session.