| Print Line Utilization (tiasl3400m000) |  |
| Use this session to print a report to show the difference between planned orders and the maximum capacity for a range of assembly lines and offline dates. You can choose to show the utilization for option combinations upon which rules are built. Related topics Assembly line station utilization
Fields | Description
Assembly Line | A set of consecutive line stations in which FAS (Final Assembly Schedule) items are manufactured. The items are manufactured by passing the items from line station to line station and by carrying out operations at each line station. An assembly line is subdivided into a number of line segments separated by buffers. An assembly line can be either a main line or a supplying line.
Print Utilization by Critical Option Combination | If this check box is selected, the report shows the utilization for option combinations on which rules are built. The maximum number of option combinations is derived from rules. Related topics Assembly line station utilization
Print Only Overloaded Option Combinations | This check box is used to determine whether only overloaded option combinations or all option combinations for the line utlization must be printed. Overloaded option combinations are option combinations that exceed the maximum number that is allowed.
Commands | Description
Print | Prints the data that you selected.