| Assembly Line - Line Segments (tiasl1541m000) |  |
| Use this session to define and display the sequence of segments for an assembly line. appropriate menu options You can start the following sessions with the selected segment as default: Simulate and Create Line Sequences (tiasl4200m000) Line Segment - Stations (tiasl1550m000) Line Segment - Line Sequence (tiasl4500m000) Line Segments (tiasl1540m000) Related topics Assembly control overview Line sequencing and rule types in Assembly Control
Fields | Description
Assembly Line | A set of consecutive line stations in which FAS (Final Assembly Schedule) items are manufactured. The items are manufactured by passing the items from line station to line station and by carrying out operations at each line station. An assembly line is subdivided into a number of line segments separated by buffers. An assembly line can be either a main line or a supplying line.
Line Segment | A set of consecutive assembly-line work centers on an assembly line between two buffers. The first buffer is the beginning of the segment, the next buffer is the first part of the next segment.
Next Line Segment | A set of consecutive assembly-line work centers on an assembly line between two buffers. The first buffer is the beginning of the segment, the next buffer is the first part of the next segment.
Next Line Segment | A set of consecutive assembly-line work centers on an assembly line between two buffers. The first buffer is the beginning of the segment, the next buffer is the first part of the next segment.
Assembly Line of Next Segment | The assembly line of the Next Line Segment. You cannot link a line segment to more than one line segments of the same assembly line. Only the last line segment of the supplying line can be linked to multiple next segments which are on different assembly lines. For more information, refer to Linking a supply line to multiple parent lines (Divergent assembly line structure) Assembly line selection - The Configuration Dependent parameter Synchronizing a supply line with mutiple parent lines Transportation time for linked assembly lines
Commands | Description
Simulate and Create Line Sequences... | Click to start the Assembly Line - Line Segments (tiasl1541m000) session.
Stations | Click to start the Line Segment - Stations (tiasl1550m000) session.
Line Sequence | Click to start the Line Segment - Line Sequence (tiasl4500m000) session.
Line Segment | Click to start the Line Segments (tiasl1540m000) session.