| Order-specific inspections |  |
| Inspection orders are used to structure the inspection of products. They are generated based on quality combinations. This means that each item to which a certain quality combination applies is inspected in the same way. You can deviate from this by means of order-specific inspections. Order-specific inspection data is the copied quality combination (that is, standard inspection data) that you can modify and change for a specific order in a specific situation. Order-specific inspection data is generated when you select the Order-Specific Inspection Data parameters in the Quality Management Parameters (qmptc0100m000) session. Procedure to generate order-specific inspections Step 1. Use the Specific Orders by Origin (qmptc0149m000) session to provide an overview of the origins and the related orders. Note: If the QM Implemented parameter in the Quality Management Parameters (qmptc0100m000) session is selected, the Specific Orders by Origin (qmptc0149m000) session can also be started from other modules. Step 2. Start the Order Specific Inspections (qmptc0550m000) session from the Specific menu in the Specific Orders by Origin (qmptc0149m000) session. You can change, add, or delete order-specific inspection orders in the Order Specific Inspections (qmptc0150m000) details session. Step 3. Start the Order Specific Inspection Lines (qmptc0151m000) session from the Specific menu in the Order Specific Inspections (qmptc0550m000) session. You can now define the order-specific inspections lines. Each line represents a characteristic that was defined in the Test Group Characteristics (qmptc0137m000) session. The order-specific inspection order is now generated. The rest of the inspection procedure is the same as that described from step 2 (drawing samples) in the Standard inspections online manual topic. Related topics Standard inspections |