| Stations (tiasl1551m000) |  |
| Use this session to list all the line stations and line buffers that are defined, in multioccurance mode, in the Line Assembly Control (LAC) module of Configurator.
Fields | Description
Station | The line station in question. A line station is part of a work center.
Station | The description of the code.
Line Segment | The segment that contains the station. Assembly lines are composed of a series of line segments. Line segments begin with a buffer that is followed by one or more line stations.
Effective Date | The first date on which the station is valid in this line segment.
Expiry Date | The last date on which the station is valid in this line segment.
Station Type | The station type on this line segment. List values: Line Station. Buffer.