| ZIP Codes by Standard Route (fmlbd0151m000) |  |
| Use this session to view and maintain zip codes for standard routes. For each standard route, the zip codes are organized in ranges by country. A range consists of the following elements: Sequence number. Country. A range of zip codes in that country. Reference address. The Sequence in Route determines the order in which the ranges are visited by the carrier. To define a range, you enter the first zip code of the range in the From ZIP Code field and the last zip code of the range in the To ZIP Code field. The carrier can pick up or deliver goods at addresses within the range. The Reference Address is the most important address of the range. Usually, this is a pooling point or a break bulk point. Note that a standard route can be a leg of a route plan. Example To define standard route AMS - PAR, Amsterdam via Brussels to Paris, you need three ranges: Sequence no. 1; The Netherlands; zip 1000AA to 1199ZZ; ref. address: Amsterdam, pooling point. Sequence no. 2; Belgium; zip 1000 to 1100; ref. address: Brussels, pooling/break bulk point. Sequence no. 3; France; zip 92974 to 92984; ref. address: Paris, break bulk point. Related topics The use of standard routes The use of route plans Planning methods
Fields | Description
Country | The country from which the range of zip codes for the standard route originates. Addresses within the zip code range can be visited by the carrier to pick up or deliver goods.
Standard Route | The standard route for which zip codes are maintained.
From ZIP Code | The first zip code of the range of zip codes for the current standard route. Addresses within the zip code range can be visited by the carrier to pick up or deliver goods.
To ZIP Code | The last zip code of the range of zip codes for the current standard route. Addresses within the zip code range can be visited by the carrier to pick up or deliver goods.
Sequence in Route | The sequence number of the zip code range. The sequence number determines the order in which the ranges are visited by the carrier.
Reference Address | The Reference Address is the most important address of the zip code range. Usually, it is a pooling point or the break bulk point.