| Calculate backflush quantity |  |
| If you report the total ordered quantity as completed, the material quantity that is issued through backflushing equals the estimated material quantity. If you report a part of the ordered quantity as completed, the material quantity to issue is calculated as follows:
    Backflushed material quantity =
    Estimated quantity x (Quantity to backflush / Quantity planned input)
The quantity-planned input is the ordered quantity, corrected for scrap and yield on the operation. The estimated quantity that appears in the Estimated Materials (ticst0101m000) session. Any scrap on the material that you do not define as a percentage but as a fixed quantity is issued all at once as soon as backflushing is carried out. You can define these scrap quantities in the following sessions: Estimated Materials (ticst0101m000) Production Planning (tisfc0110m000) Related topics Backflushing procedure Scrap and yield Backflushing |