| # Divergent supply line structure New in Infor LN 10 In Infor LN 10, you can create a divergent assembly line structure in Assembly Control. In the divergent assembly line structure, one supply line is linked to multiple main assembly lines. For more information, refer to Linking a supply line to multiple parent lines (Divergent assembly line structure). Related topics Assembly line selection— Configuration Dependent parameter Synchronizing a supply line with mutiple parent lines Transportation time for linked assembly lines |