| # Inspection methods for materials If the QM Implemented Material (BOM) check box in the Quality Management Parameters (qmptc0100m000) session is selected, you can use Quality to check the materials for production orders. You can define the quality requirements for each material. If you select the Material (BOM) check box in the Quality Management Parameters (qmptc0100m000) session, you can open the Order Specific Test Procedures (qmptc0149m000) session from the Estimated Materials (ticst0101m000) session. Possible scenarios to implement quality for the materials: The materials are inspected, but the inspection orders have no impact on the production orders (method A). You must inspect the materials, before you can issue them for a production order (method B). The Blocking Method field in the Order Inspections (qmptc1120m000) session determines method that you can use. Infor LN uses method A, if the Blocking Method field has the value Continue. Infor LN uses method B, if the Blocking Method field has the value Block. Infor LN determines the value of these fields on the basis of the data you enter in the following sessions: Testing Combinations (qmptc0111m000) Order Specific Test Procedures (qmptc0149m000) Related topics Manufacturing operations Quality control of end products Quality control of materials |