Log configuration

Use this page to specify the log configuration for the JCA Connectivity plug-in. When the log configuration is changed and saved, the new log configuration will be effective immediately.

The log configuration is effective for all Connection Points defined in the Infor ERP LN Connectivity Preferences dialog.

Related topics

- Introduction
- To configure connection points
- To define the log configuration

Fields
Fields | Description
Log file location
Location | The name and location of the log file of ERP LN Connectivity. The log file must be located on the computer that runs the client application. To add the functionality to log to a file, select the (System log file) check box and enter the path and the name of the log file. Important! The log file name must contain a .log extension. The log file must be writable. You must enter an absolute path. The log file should not be empty. There must be permissions to write a file at te specified location. The directory in the given location should exist, the file can be new.
(System log file) | This checkbox enables or disables the logging to a log file. If this check box is cleared, the Location text field is disabled and logging to a file is disabled. If this check box is selected, the Location text field is enabled, and validation on the Location text field is enabled. Logging to a file is then enabled again. Click Browse (when the System log file is enabled), to select a directory where the log file should be stored. After selecting the directory, you must add a log file name (with a .log extension).
Application log level
(supported log levels) | The log level for the entire Infor ERP LN Connectivity plug-in. Select one of the following options:
Log level | Description
Error | Designates error events that can still allow ERP LN Connectivity to continue running. The error message indicates that parts of the application are not working or working incorrectly. The Error level also includes the logging of fatal errors..
Info | Designates informational messages that highlight the progress of the application at coarse-grained level. Such informational messages include, for example, the initialization of a configuration or the end of a long import process. The Info level includes Error logging.
Debug | Designates fine-grained informational events that are most useful to debug ERP LN Connectivity. Use this level only for developing purposes to follow the program execution. The Debug level includes the Info logging.

Commands
Commands | Description
OK | Saves the preferences in the standard directory where the log configuration file is stored.

| Send Us Your Feedback About this Help Page