Log configuration

Use this page to specify the log configuration for the JCA Connectivity plug-in. When the log configuration is changed and saved, the new log configuration will be effective immediately.

The log configuration is effective for all Connection Points defined in the Infor ES JCA Connectivity dialog.

Related topics

- Introduction
- To configure connection points
- To define the log configuration

Fields
Fields | Description
Log file location
Enable logging | This check box enables or disables the logging to a log file. If this check box is cleared, the Location field is disabled and logging to a file is disabled. If this check box is selected, the Location field is enabled, and validation on the Location field is enabled. Logging to a file is then enabled. To select a directory to store the log file, when logging is enabled, click Browse. After you select the directory, you must add a log file name with a .log extension.
Location | The name and location of the log file of LN Connectivity. The log file must be located on the computer that runs the client application. To add the functionality to log to a file, select the Enable logging check box and enter the path and the name of the log file. Important! The log file name must contain a .log extension. The log file must be writable. You must enter an absolute path. The log file should not be empty. There must be permissions to write a file at the specified location. The directory in the given location should exist; the file can be new.
Application log level
(supported log levels) | The log level for the entire Infor LN Connectivity plug-in. Select one of the following options:
Log level | Description
Error | Designates error events that can still allow LN Connectivity to continue running. The error message indicates that parts of the application are either not working or incorrectly working. The Error level also includes the logging of fatal errors.
Info | Designates informational messages that highlight the progress of the application at coarse-grained level. Informational messages include, for example, the initialization of a configuration or the end of a long import process. The Info level includes Error logging.
Debug | Designates fine-grained informational events that are useful to debug LN Connectivity. Use this level only for developing purposes to follow the program execution. The Debug level includes the Info logging.
Limit file size
On size | If this check box is selected, you can specify settings to limit the disk space occupied by the log files.
Maximum size log file (in Mb) | If a log file exceeds the specified size, a copy of the log file is created and the original file is cleared. In this way, a series of log files is generated.
Maximum number of log files | Specify the maximum number of log files to be generated. If the last log file in the series exceeds the maximum size, the logging continues in the first log file. In this way, the log file series is reused.
On time | If this check box is selected, you can specify settings to periodically clean the log file. Click one of the corresponding options to specify how often the file must be cleaned.

Commands
Commands | Description
OK | Saves the preferences in the standard directory where the log configuration file is stored.

| Send Us Your Feedback About this Help Page