| # Maintenance Trigger Sets (tsmdm0168m000) Use this session to create and maintain maintenance trigger sets. Note To create numeric maintenance trigger set, select the New Numeric Maintenance Trigger Set option. To create alphanumeric maintenance trigger set, select the New Alphanumeric Maintenance Trigger Set option. Related topics Service inspections and preventive maintenance scenarios Maintenance Trigger Set The set of maintenance triggers that is used to trigger maintenance notifications when performing inspections. Description The description or name of the code. Measurement Type The measurement type for which maintenance trigger is defined. Note If the maintenance trigger type is Alphanumeric then the measurement type must be of type Condition Based Alphanumeric. If the maintenance trigger type is Numeric then the measurement type must be of type Counter or Condition Based Numeric. Description The description or name of the code. Norm Value (Numeric) The norm value for the numeric measurement type. Norm Value (Alphanumeric) The norm value for the alphanumeric measurement type. Note The norm value is defaulted from the Alphanumeric Measurement Values (tsmdm0166m000) session. |