| # Routing New in Infor LN 10.2.1 It is now possible to automatically propagate a 'move' or 'swap' of assembly order on a specific line segment to previous and succeeding connecting line segments. A new parameter was added to the existing Reschedule Assembly Orders (tiasl4220m000) session. Related topics Assembly line selection— Configuration Dependent parameter Synchronizing a supply line with mutiple parent lines Transportation time for linked assembly lines |