| # Displaying Assembly Lines Assembly lines consist of a series of line segments. Segments in turn consist of a buffer and one or more line stations, until the next buffer. The calendar that is linked to Calendar Code, together with the Availability Type that is defined in the ASC parameters, determines the working hours of the assembly line. You can view which line segments belong to the assembly line in the Assembly Line - Line Segments (tiasl1541m000) session. You can view which lines stations belong to the assembly line in the Line Segment - Stations (tiasl1550m000) session. Menu options The appropriate menu contains various options to start the following sessions related to assembly lines: Close Assembly Lines (tiasc7220m000) Build Assembly Part Allocation (tiasc7240m000) Backflush Requirements (tiasc7241m000) Offset Line Station Orders (tiasl4230m000) Purge State-independent ASC Data (tiasl1210m000) Purge State-dependent ASC Data (tiasl1200m000) Purge and Renumber Sequences (tiasl4201m000) Assembly Line - Line Segments (tiasl1541m000) Assembly Line - Status (tiasc7520m000) Assembly Line - Line Mix (tiasc2501m000) Assembly Line - Line Utilization (tiasl3500m000) Assembly Line - Assignments (tiasc5510m000) The options on the File menu allow you to start the following print sessions: Print Assembly Line Structure (tiasl1430m000) Print Costing by Assembly Order or Assembly Line (tiasc7411m000) Print Financial Transactions by Assembly Line (tiasc7414m000) Related topics Assembly control overview Assembly order costing Line sequencing and rule types in Assembly Control |