| # Displaying Assembly Line - Assignments and Line Stations Assignments are either defined for a whole assembly line, or for a particular line station. Assignments defined for an assembly line, called Line Level Assignment, actually consists of a set of line station level assignments. The line level assignment defines when the line station level assignments are active, and defines a cycle time for them. This session displays all the line station level asignments that are defined for a specific line level assignment on a line station. Note Two types of line level assignments exist. Average assignments Average assignments only define an average cycle time, that is applicable for the whole line, and are not linked to line station level assignments. Nonaverage assignments Line station level assignmets are only linked to nonaverage line level assignments. The data displayed in this session is in effect when the assignment to which the data belongs, which is displayed at the top of this session, is active. The line level assignments are displayed in the Assembly Line - Assignments (tiasc5510m000) session. Related topics Assembly control overview Assembly line station utilization Assembly assignment |