| # Maintenance Triggers by Trigger Set (tsmdm0668m000) Use this session to create numeric and alphanumeric maintenance triggers for the specific maintenance trigger set. Note You can define maintenance triggers with a trigger message, default recommendation and default follow-up activity. Related topics Service inspections and preventive maintenance scenarios Maintenance Trigger Set The maintenance trigger set that holds the maintenance triggers applicable for the measurement type. Description The description or name of the code. Measurement Type The measurement type for which maintenance trigger is defined. Note If the maintenance trigger type is Alphanumeric then the measurement type must be of type Condition Based Alphanumeric. If the maintenance trigger type is Numeric then the measurement type must be of type Counter or Condition Based Numeric. Description The description or name of the code. Norm Value (Numeric) The norm value for the numeric measurement type. Unit The unit of the norm value. Norm Value (Alphanumeric) The norm value for the alphanumeric measurement type. |