| # Process EBOM Changes (tiedm3205m000) Use this session to generate single-level EBOMs for the revisions which have been generated or modified by MBCs. The single-level EBOMs are based on the E-items from the E-Item by MBC (tiedm3122m000) session and on the order lines from the MBC Action (tiedm3120m000) session. Related topics Calculating net quantity Engineering data management summary Changing EBOMs - Automatic procedure Finalizing engineering data Selection Range MBC Number Enter a range of MBCs, whose changes to EBOMs you want to process. Option Approve New Revisions by Engineering If this check box is selected, the status of new revisions is automatically set to Approved by Engineering after their EBOMs have been generated. If this check box is cleared, you must approve revisions using the Engineering Item Revision (tiedm1100m000) session. Create Links to Documents attached to Component and Revision If this check box is selected, all documents attached to the component or engineering item revision in Data Management, are copied to the EBOM. Related topics Object Data Management Components Modifying Engineering Item Revision |