| # Process backflushed materials LN backflushes the materials linked to the operations for which quantities are reported as completed. If a production order has no operations, LN backflushes all materials. For details about the calculation of the quantities to issue through backflushing, see Calculate backflush quantity. You can see the result of backflushing materials in the Production Orders (tisfc0101s000) session. LN subtracts the backflushed material quantity from the Subsequent Delivery field and adds the same quantity to the To Issue field. The corresponding warehousing order is immediately initiated. Note LN does not decrease the value of the Subsequent Delivery field below zero. LN also prints the results of backflushing materials in a report. Related topics Backflushing procedure Link materials to operations Calculate backflush quantity Overview of material issue Backflushing |