| # Print Test Plan by Standard Test Procedure (qmptc0412m000) Use this session to print the test plans for a range of quality IDs. Standard Test Procedure The code to which data is linked that is necessary to check the quality requirements of an item. Since one standard test procedure can be used for a group of products that require the same quality standards and tests, a standard test procedure can considerably reduce time. Quality ID The code to which data is linked that is necessary to check the quality requirements of an item. Since one standard test procedure can be used for a group of products that require the same quality standards and tests, a standard test procedure can considerably reduce time. Validation Date The date that the quality ID(s) must be valid. A quality ID is valid when inspection data can be generated. This means that: The quality ID has at least one test group ( Test Groups (qmptc0136m000) session) At least one test group has a valid combination of an aspect and characteristic ( Test Group Characteristics (qmptc0137m000) session). Note When you entered Algorithm in the Method field, a characteristic is only valid when all combinations of an aspect and characteristic needed by the algorithm are present and valid. The current date falls between the effective date and the expiry date of the combination of an aspect and characteristic of the quality ID ( Standard Test Procedure Characteristics (qmptc0115m000) session) Only one test type can have destructive tests ( Characteristic Tests (qmptc0105m000) session). Note The total sample percentage of the test groups with destructive tests can be 100% at the most. Text If this check box is selected, the text that are linked to the quality IDs/test plans are printed in the report. |