| Possible values |  |
| All Available Lines All the PBOM lines are replaced by the EBOM lines and by non-EBOM lines. The latter are lines from a standard PBOM that are copied to a project (using the copy method NonProj Item to Proj Item in the EBOM Copy Data (tiedm1120m000) in the session). Only Corresponding Pos. Lines in the PBOM with the same position numbers as the EBOM are replaced by the corresponding EBOM lines and non-EBOM lines. The other PBOM lines remain unchanged. Corresp. and Linked Pos. The following lines in the PBOM are replaced by EBOM lines and non-EBOM lines: Lines in the PBOM that have the same numbers as EBOM lines. Lines in the PBOM that have numbers that differ from the EBOM line numbers, in which case the Link with EDM check box in the Bill of Material (tibom1110m000) session must be selected, and the numbers were created by previous finalizing actions on the engineering data. The other lines from the PBOM remain unchanged. These lines are not engineering-related (for example, packing materials). In this way, you can make a clear distinction in PBOMs between engineering-related components and logistics components which do not relate to engineering. |