| Work Center Utilization by Day (tisfc1506m000) |  |
| Use this session to display an overview of capacity utilization of a work center for one day. You can see, for each order, the time and quantity that it is planned. You can only use this session if you have selected Automatic or Manual in the Update Method Day Utilization field in the Shop Floor Control Parameters (tisfc0100s000) session. Note If you have started this session by zooming, you can only find and select a record. Related topics Production orders - functional overview How to calculate available capacity To use an overview session
Fields | Description
Work Center | The work center for which you want to see a summary of what capacity requirement are planned for that day. To see utilization for a shared work center, use the Shared Work Center Utilization (tisfc1510m000) session.
Description | The work center for which you want to see a summary of what capacity requirement are planned for that day. To see utilization for a shared work center, use the Shared Work Center Utilization (tisfc1510m000) session.
Normal Capacity | The average capacity of a machine or work center that is used as the basis for the capacity utilization.
Production Date | The day for which you want to see a summary of what capacity requirement are planned.
Available Cap | The available capacity (hours) of the employee working at the work center for the day in question. Related topics How to calculate available capacity
Start Time | The start of the period for which you want to see what capacity has been planned.
Production Order | The code of the planned production order.
Item | The item produced in the operation.
Routing | The sequence of operations required to manufacture an item. For each operation, the task, machine, and work center are specified, as well as information about setup time and cycle time. Note If no routing is displayed, there are no estimated production costs defined for the production order.
Operation | The code of the operation planned for the work center.
Machine | The machine with which the operation is carried out.
Quantity Planned | The quantity of items you plan to produce in this operation on this date, including items lost to scrap and low yield.
Man Hours | The man hours needed to carry out the operation Related topics Calculating man/machine hours
Physical Location | The location where the order is processed.
SFC Order Group | The group of orders to which the order belongs. Related topics Order grouping
Machine Hours | The machine hours needed to carry out the operation Related topics Calculating man/machine hours
Normal Capacity | The average capacity of a machine or work center that is used as the basis for the capacity utilization.
Available Cap | The available capacity (hours) of the machine working at the work center for the day in question. Related topics How to calculate available capacity
Commands | Description
Production Planning | Starts the Production Planning (tisfc0110m000) session.
Build Utilization | Starts the Build Utilization (tisfc0201m000) in which you can update the plans from the Enterprise Planning module. All the utilization data is deleted and is regenerated using the production quantity and date data in the Production Planning (tisfc0110m000) session. This cannot be done for line work centers. You must select Automatic in the Update Method Day Utilization field and Automatic in the Update Method Week Utilization field in the Shop Floor Control Parameters (tisfc0100s000) session before you can use this option.