| Remix/Sequence Parameters (tiasl4110m000) |  |
| Use this session to maintain and display the remixing/sequencing parameters for a user. The parameters are displayed per segment. You can only edit the data for yourself. If you want to view data for another user, click the Find button. Note You can define more general parameters in the Assembly Control Parameters (tiasc0100m000) session. Related topics Line sequencing and rule types in Assembly Control Assembly control overview
Fields | Description
User | The user's logon code. You can only edit data for yourself.
Line Segment | The parameters are only valid for this line segment.
Line Segment | Paramters are only valid for a specified line segment.
Number of Local Runs | The number of times ERP LN carries out a calculation to determine the best sequence in the line segment.
Number of Global Runs | The number of times ERP LN carries out a calculation to determine the best sequence order in the line segment. In the Remix Line Mix (tiasl3220m000) session, this parameter is taken into consideration to determine the number of times the process of remixing must be carried out to arrive at a better line mix.
Local Maximum Swap Distance | The maximum number of positions between orders that you swap in the Simulate and Create Line Sequences (tiasl4200m000) session. If you increase the swap distance, the quality improves because more swaps are possible. However, if you increase the swap distance, each sequencing simulation run takes longer.
Global Maximum Swap Distance | The maximum number of positions between orders that you swap in the Simulate and Create Line Sequences (tiasl4200m000) session. If you increase the swap distance, the quality improves because more swaps are possible. However, if you increase the swap distance, each sequencing simulation run takes longer.
Local Run Count | The maximum number of attempted swaps per sequencing run. ERP LN checks to see whether this number has been exceeded after each series of swaps, determined by the maximum swap difference and number of orders. When the value of this field has been exceeded, one sequencing run has been completed.
Global Run Count | The maximum number of attempted swaps per sequencing run. ERP LN checks to see whether this number has been exceeded after each series of swaps, determined by the maximum swap difference and number of orders. When the value of this field has been exceeded, one sequencing run has been completed. In the Remix Line Mix (tiasl3220m000) session, this parameter is taken into consideration. It represents the maximum number of attempted swaps per reximing run.
Local Non-improvement Count | The number of times that ERP LN swaps orders in the selected segment without any improvement to cost before stopping the sequencing run.
Global Non-improvement Count | The number of times that ERP LN swaps orders in the selected segment without any improvement to cost before stopping the sequencing run. In the Remix Line Mix (tiasl3220m000) session, this parameter is taken into consideration. It represents the number of times the orders are swapped in the selected segment without any improvement to cost before stopping the remixing run.