| Print Kanban Labels (tirou2402m000) |  |
| Use this session to print Kanban labels. In this session, you must define (ranges for) a combination of item, routing and operation. For each operation in a routing, a work center exists. With this session, you can print kanban labels to pass intermediate products on to the next work center in a routing. Note You can define kanban related information in the Routing Operations (tirou1102m000) session. Related topics Labels in Manufacturing To use From and To fields
Fields | Description
From Item | An item that occurs in any module of Manufacturing. It is a purchased, manufactured, or generic item that is used in a generic/production bill of material or in a generic/production routing.
To Item | An item that occurs in any module of Manufacturing. It is a purchased, manufactured, or generic item that is used in a generic/production bill of material or in a generic/production routing.
Routing | The sequence of operations required to manufacture an item. For each operation, the task, machine, and work center are specified, as well as information about setup time and cycle time.
Routing | The sequence of operations required to manufacture an item. For each operation, the task, machine, and work center are specified, as well as information about setup time and cycle time.
Operation | One of a series of steps in a routing that are carried out successively to produce an item. The following data is collected during a routing operation: The task. For example, sawing. The machine used to carry out the task (optional). For example, sawing machine. The place where the task is carried out (work center). For example, woodwork. The number of employees required to carry out the task. This data is used to compute order lead times, to plan production orders and to calculate cost prices.
Operation | One of a series of steps in a routing that are carried out successively to produce an item. The following data is collected during a routing operation: The task. For example, sawing. The machine used to carry out the task (optional). For example, sawing machine. The place where the task is carried out (work center). For example, woodwork. The number of employees required to carry out the task. This data is used to compute order lead times, to plan production orders and to calculate cost prices.
Reference Date | A user definable date that ERP LN uses to check whether an operation is valid. An operation is valid on the reference date if it falls within the operation's effective date and expiry date, as defined in the Routing Operations (tirou1102m000) session. Note You can only print kanban labels for valid operations.
Label Layout | If you use Kanban labels to trigger supply on the shop floor, the label layout entered in this field determines the format of the labels. You can define the use of kanban labels in the Print Kanban Labels (tirou2402m000) session. Note The default value in this field equals the value defined in the Routing Parameters (tirou0100m000) session. Related topics Labels in Manufacturing
Connect as phantom routing | If the item range includes a phantom item, you can select this check box to connect the combination of the item, routing and operation as a phantom routing to an operation of an item situated on a higher BOM level. As a result, the kanban labels are printed for the selected (joined) operation in the (joined) routing of the (joined) item in the higher BOM level. Related topics Item to Join. Routing to Join. Operation to Join. Phantoms
Routing to Join | Select the routing that must be linked to the phantom routing. Related topics Phantoms
Operation to Join | Select the operation that must be linked to the phantom routing. Related topics Phantoms
Item to Join | Select the item, situated on the higher BOM level, that must be linked to the phantom routing. Related topics Phantoms
Commands | Description
Print | Prints the entered selection.