| To set up inspection methods for materials |  |
| To set up inspection methods for materials If the QMS Implemented for Material (BOM) check box in the Quality Management Parameters (qmptc0100m000) session has been selected, you can use the Quality Management package to check the materials for production orders. You can define the quality requirements for each material in the Quality Management package. If you select the Material (BOM) check box in the Quality Management Parameters (qmptc0100m000) session, you can zoom to the Specific Orders by Origin (qmptc0149m000) session from the Estimated Materials (ticst0101m000) session. You can choose between two methods which determine the interactions between the Shop Floor Control module and the Quality Management package with respect to materials: The materials are inspected, but the inspection orders have no direct effect on the production orders (method A). You must inspect the materials, before you can issue them to a production order (method B). The Blocking Method for Inspections field in the Standard Orders by Origin (qmptc1120m000) session determines which of the methods mentioned above will be used. ERP LN applies method A, if the Blocking Method for Inspections field has the value Continue. ERP LN applies method B, if the Blocking Method for Inspections field has the value Block. ERP LN will determine the value of these fields on the basis of the data you enter in the following sessions: Quality Combinations (qmptc0111s000) Specific Orders by Origin (qmptc0149m000) Related topics Using QM for manufacturing operations Using QM for products of production orders Using QM for materials of production orders |