| # To set up inspection methods for operations Setting up inspection methods for operations If the Routing (TI) check box in the Quality Management Parameters (qmptc0100m000) session has been selected, you can use Quality Management to check the products of operations. You can define the quality requirements for each operation in the Quality Management package. If you select the Routing (TI) check box in the Quality Management Parameters (qmptc0100m000) session, you can zoom to the Specific Orders - By Origin (qmptc0149m000) session from the Production Planning (tisfc0110m000) session. You can choose between four methods which determine the interactions between the Shop Floor Control module and the Quality Management package with regard to the routing operations: You inspect the subassemblies, but the operations are in no way affected by the inspection orders (method A). You must inspect the subassemblies before you can report an operation as complete. However, you are free to report any quantity as complete or as rejected, regardless of the results of the tests (method B). You must inspect the subassemblies before you can report quantities as complete or rejected. The inspections result in recommendations for the quantities completed and rejected (method C). You must inspect the subassemblies before you can report quantities as complete or rejected. The results of the inspections determine the quantity completed and rejected. You cannot modify these quantities (method D). The following fields determine which of the methods mentioned above will be used: Blocking Method QM Only Recommends You can find these fields in the Standard Orders - by Origin (qmptc1120m000) session. LN applies method A, if the following conditions are met: Blocking Method = Continue The QM Only Recommends check box is selected LN applies method B, if the following conditions are met: Blocking Method = Block on Compl. Operation The QM Only Recommends check box is selected LN applies method C, if the following conditions are met: Blocking Method = Block on Operation The QM Only Recommends check box is selected LN applies method D, if the following conditions are met: Blocking Method = Block on Operation The QM Only Recommends check box is cleared LN will determine the value of these fields on the basis of the data you enter in the following sessions: Quality Combinations (qmptc0111m000) Specific Orders - By Origin (qmptc0149m000) Related topics Using QM for manufacturing operations Using QM for products of production orders Using QM for materials of production orders |