| # Offset Line Station Orders (tiasl4230m000) Use this session to offset line station orders (LSOs). Offsetting is the process of calculating the start times and end times. To have accurate start times and end times is important, for example, for the allocation of materials. Related topics Assembly control overview Line sequencing and rule types in Assembly Control Assembly orders From The assembly lines on which the assembly orders must be offset. Offline Date To The date that determines which orders are offset. Assembly orders you want to offset, must have an offline date before or on this date. Planned Assembly Orders If this check box is selected, Planned assembly orders are offset. Offsetting for planned assembly orders is performed on line segment level. Sequenced Assembly Orders If this check box is selected, Sequenced assembly orders are offset. Offsetting for sequenced assembly orders is performed on line station level. Offset Calculates the start time and the end time for each line-station order, and to offset the orders according to their start times and their end times. Messages Displays error messages, such as line station orders whose requirements have not been backflushed or WIP transfers that cannot be created. |