| # Global Update of Order-Specific Inspection Data (qmptc0250m000) Use this session to add, update, or delete order-specific data collectively for a range of origin orders. If the Update Mode field has the value: Add: new order-specific inspection data will be generated from the master data. Update: the existing inspection data will be deleted, and then new inspection data from the master data will be generated. Delete: order-specific inspection data will be deleted. Note Usually you will only define a selection range when you choose just one origin (unless by chance that specific selection range applies to more origins). If you select more than one origin, without a selection range, all origin orders will be updated. Related topics Order-specific inspections Update Mode You can change order-specific inspection data in various ways: 1. An integrated module or package to which an (inspection) order is related. In the Quality Management package an inspection order can relate to various origins: Origin of Inspection Operation One of a series of steps in a routing that are carried out successively to produce an item. The following data is collected during a routing operation: The task. For example, sawing. The machine used to carry out the task (optional). For example, sawing machine. The place where the task is carried out (work center). For example, woodwork. The number of employees required to carry out the task. This data is used to compute order lead times, to plan production orders and to calculate cost prices. Operation One of a series of steps in a routing that are carried out successively to produce an item. The following data is collected during a routing operation: The task. For example, sawing. The machine used to carry out the task (optional). For example, sawing machine. The place where the task is carried out (work center). For example, woodwork. The number of employees required to carry out the task. This data is used to compute order lead times, to plan production orders and to calculate cost prices. |