| # Capacity Flows between Departments (bptmm2525m000) Use this session to display the capacity flows recorded by LN. Related topics Capacity flows Capacity Flow Type In LN, the following types of capacity flow exist: Contracting-In Contracting-Out Input Capacity Flow Output Capacity Flow Department from/to Capacity Flows The code of the department involved. Task An activity to manufacture or repair an item. For example, sawing, drilling, or painting. A task is carried out on a work center, and can be related to a machine. Time Unit The physical quantity in which an item or good is managed. For example, a quantity of wood can be expressed as a length by using the unit of one meter, or as a volume by using the unit of one cubic meter. Labor Time The amount of time spent by an employee on a task or activity. Machine Time A department's total machine time spent on a specific order or a specific project in a given year and period. Labor Costs Costs related to tasks performed by employees. Labor costs are based on the employee's labor rate and the number of hours spent on a task or activity. Machine Costs The costs of using a machine to carry out an operation. Overhead Costs The overhead cost. Year/Period The year the hours are booked. / The period code. |