| # Copy or Skip BOM Line (tipcs2235m000) You can use this subsession to copy or skip a BOM line during an interactive copy action. Manuf. Item The code of the manufactured item. Position A reference number identifying a specific combination of manufactured and component items in a bill of material. The position number is subdivided by sequence numbers that are used to refer to usage of a component between particular dates. / The BOM sequence number allows you to define more than one component item for each position. These interchangeable components can have different dates when they are valid. LN also uses sequence numbers when you replace items in BOMs. Example Say, you make bicycles and use frames that you buy from supplier A until August. However, after August you will use identical frames that you buy from supplier B. Do not use a new BOM position number for the second frame. Instead, use a new sequence number. Item A purchased item, material, subassembly, or finished product that is normally available. All items that are not built according to customer specification for a specific project are defined as standard items. Opposite term is customized item. A standard item can have the following order policies: Anonymous To Order Order Policy The order parameter that controls the way an item is produced or ordered. This can be: Anonymous, the item is produced or purchased independent of customer orders. To order, the item is produced or purchased only if customer orders exist for the item. Manuf. Item A non-existing manufactured item to which the source item is copied in order to create a new manufactured item. Item This is the item the BOM line is to be copied to. |