| # Print Quality ID - Characteristics (qmptc0415m000) Use this session to print (a range of) characteristic s that are linked to (a range of) quality ID s. You can select whether the report contains header data or detailed data. Related topics Quality ID's and quality combinations Quality ID The code to which data is linked that is necessary to check the quality requirements of an item. Since one quality ID can be used for a group of products that require the same quality standards and tests, a quality ID can considerably reduce time. Quality ID The code to which data is linked that is necessary to check the quality requirements of an item. Since one quality ID can be used for a group of products that require the same quality standards and tests, a quality ID can considerably reduce time. Aspect A part of an item. For example, a bolt can have the aspects head and tail. An aspect can have one or more characteristics. For example, a head can have a diameter and a length, and a tail can have a diameter and a color. Aspect A part of an item. For example, a bolt can have the aspects head and tail. An aspect can have one or more characteristics. For example, a head can have a diameter and a length, and a tail can have a diameter and a color. Characteristic A reference to a particular quality or distinctive mark of an item or an item part/component. For example, diameter, length, weight. Characteristic A reference to a particular quality or distinctive mark of an item or an item part/component. For example, diameter, length, weight. Sequence The sequence number of the inspection order on the basis of which characteristics are tested on different samples. Sequence The sequence number of the inspection order on the basis of which characteristics are tested on different samples. Print Characteristic Text If this check box is selected, the text that is linked to the characteristic in the Characteristics (qmptc0115m000) session is included in the report. |