| # Engineering Item Revision (tiedm1100m000) Use this session to modify and define revisions of E-items. You can, for example: Enter data for revisions of engineering items. Import revision data from a CAD application. Change the revision status of an E-item revision. Related topics Engineering data management summary Engineering items Import CAD application data with the Exchange module Overview of reference designators Integration Manufacturing and Document Management Engineering Item The E-item for which you want to maintain revisions. Manual Revision Numbering If this check box is selected, you can enter the revision number manually when you create new revisions. If you change the revision numbering mode in between, for example, from manual to automatic, the next highest number for the current revision series for the E-item is generated. Engineering Item Revision The engineering item's revision for which you are defining a bill of material (BOM). Related topics Engineering items Status The status of the revision. Allowed values Engineering Item Revision Status Creation Date The date on which the revision was created. BOM Quantity BOM quantity. Unit Set A group of unit codes that can be linked to standard or customized items, or to item defaults. In a unit set, you can indicate the physical quantities that can be used for the item, in which modules, and for what purposes. Material What the E-item revision is made of, for the current revision. For example, paper, plastic, wood. Size How large the E-item revision is, for the current revision. For example, 200 mm x 1 meter. Norm Standard The company, national, or international standard to which the E-item revision conforms (or must conform), for the current revision. For example, ISO 8601, NEN 3140, BS 1383. Unit Unit of measurement, such as meter, kilogram, or piece. Weight Unit Unit of measurement for weight, such as a kilogram. Weight The weight of the revision, entered in the units that you have defined in the Weight Unit field. Engineer The employee who is responsible for supervising the design of the revision. Engineer Displays the value entered in the Employee field in the Employees - General (tccom0101m000) session, from which you select the value for the Engineer field. MBC The mass BOM change used to control the revision. Related topics Engineering data management summary To change EBOMs - Automatic procedure In process by Change Management If this check box is selected, an approval procedure for the E-item revision has started in Data Management. You must first complete the approval procedure before you can approve the revision for production. Effective Date The date and time that the revision becomes effective. You can change this date manually to any future date. If you have multiple revisions that have the In-design status, you can schedule the effective date for all these revisions. If you approve an E-item revision that has an effective date for production that is before the current date, the effective date is automatically set to the Approved by Production date. If the revision is finalized, the effective date of the revision for the parent E-item is taken as the effective date for the PBOM lines. So the desired effective date for the PBOM lines must be set here. Expiry Date If the revision has the Approved by Production status, the Expiry Date field is empty, and you can set this date manually. When a new revision is created with an effective date before the expiry date of the previous revision the expiry date of the previous revision is set to the effective date of this new revision. You cannot change the expiry date if: The status of the revision is not Approved by Production. The revision has been Approved by Production, but the Expiry Date field is filled. Related topics Engineering items Approved by Engineering Date The date that the revision was Approved by Engineering. Once a revision is Approved by Engineering it cannot be deleted, only canceled and archived. Approved by Production Date The date that the revision received the Approved by Production status. Date from CAD The date that the revision was imported from a CAD application. Related topics Import CAD application data with the Exchange module Text If this check box is selected, a text is present. To enter a new text, or edit an existing text, click the Text button. Freeze Click to set the revision's status to Frozen. You can only do this for revisions whose status is In-design. Reset Revision Status Click to set the revision's status to In-design. You can only do this for revisions whose status is Frozen. If the status is greater than Frozen and you want to change the design, you can cancel the revision and make a new one. Approve by Engineering Click to set the revision's status to Approved by Engineering. You cannot change the status to Approved by Engineering if the revision is created by an MBC for which EBOM changes are not yet processed. You can only do this for revisions whose status is: Frozen In-design Approve by Production Click to set the revision's status to Approved by Production. You cannot change the status to Approved by Production if the revision is created by an MBC for which EBOM changes are not yet processed. You can only do this for revisions whose status is: Approved by Engineering. In-design Cancel Revision Click to set the revision's status to Canceled. You can only do this for revisions whose status is Approved by Engineering: In-design revisions can be deleted Approved by Production revisions can be archived Canceled revisions can be archived. EBOM Click to start the Engineering BOM (tiedm1110m000) session. Relationships Click to start the Engineering Item - Item Relationship (tiedm1101m000) session. Reference Designators by Engineering Item Click to start the Reference Designators by Engineering Item (tiedm0120m000) session, in which you can view, maintain, or add reference designators for a specific engineering item revision. |